Stepwedge – User Documentation

|  |  |  |  |
| --- | --- | --- | --- |
| Function | Line (approx) | Issue | Resolved |
| stepwedge | 206 | Assume 18x24 films need rotating – depends how films have been digitised? In general, check assumptions about how films are oriented (in segmentation algorithm I’ve tried to do this automatically – implement that here?) |  |
| stepwedge | 213 | Median filter with a 3x3 window – sensible enough but ever been tested? |  |
| markerdetect | 48 | Number of rows at top/bottom of image in which to search for markers is hardcoded (show\_rows = 600) – dangerous if image resolution changes. Make argument and set to default to be a % of image height? |  |
| find\_marker | 44 | Size of box about user select position is hardcoded (box\_size = 100) - angerous if image resolution changes. Make argument and set to default to be a % of image size? |  |
| find\_marker | 60 |  |  |